**Culvert Bid 2025 – Tabulation**

|  |  |  |  |
| --- | --- | --- | --- |
| Company Name | Company Name | Company Name | Notes |
| Jensen Bridge & Supply Company400 Stoney Creek DriveP.O. Box 151Sandusky, Michigan 48471Jim Nuttall jimn@jensenbridge.com810-648-3000 | St. Regis Culvert Inc. 202 Morrell StreetCharlotte, Michigan 48813Brian Caldwell517-588-1737bcaldwell@stregisculvert.com | Cadillac Culvert, Inc.5305 Highway M-115Cadillac, Michigan 49601Darin Hower231-775-3761darin@cadillacculvert.com |  |
| 12” – 16ga – 8.70/ft15” – 16ga – 10.50/ft18” – 16ga – 12.87/ft18” – 14ga – 16.93/ft24” – 16 ga – 16.69/ft24” – 14ga – 22.44/ft30” – 14ga – 28.56/ft36” – 14ga – 33.52/ft | 12” – 16ga – 7.00/ft15” – 16ga – 8.52/ft18” – 16ga – 10.80/ft24” – 16 ga – 13.87/ft36” – 14ga – 27.00/ft48” – 12ga – 48.75/ft1 ft band is 1.65 x $/ft2 ft band is 2 x $/ft | 12” – 16ga – 6.97/ft – band 11.5015” – 16ga – 8.44/ft – band 13.9318” – 16ga – 10.14/ft – band 16.7324” – 16 ga – 14.12/ft – band 23.3024” – 14ga – 22.44/ft – band 37.0330” – 14ga – 28.05/ft – band 55.5436” – 14ga – 33.66ft – band 66.6512”-24” bands are 12” width30” and larger bands are 24” width |  |

Moved to accept all bids and to authorize staff to purchase in the best interest of the Crawford County Road Commission